|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Assessed By:** | | **Kevin Lovett** | | | | | | | | | **Risk Assessment No:** | | | | | **RA02** | |
| **Hazard Identified:** | | **Painting** | | | | | | | | | **Date Reviewed:** | | | | | **June 2025** | |
|  | | | ***A*** | | | | | ***B*** | | | | ***C*** | | | | ***D*** | |
| **Who’s at Risk?** | | | | | **Severity** | | | | **Likelihood** | | | | **Risk Rating** | |
| **E** | | **C** | **P** | | **3** | **2** | **1** | | **3** | **2** | | **1** | **B x C = D** | |
| **🗸** | |  |  | |  | **🗸** |  | |  | **🗸** | |  | **4** | |
| Risk Assessment Ratings | **6-9 High Risk** | | | | | | **4 Medium Risk** | | | | | | | **1-3 Low Risk** | | | |
| **Key** | | | | | | | | | | | | | | | | | |
| **A**  E = Employees  C = Contractors  P = Public / 3rd parties | | | | **B**  3 = Death or Major injury  2 = Reportable injury  1 = Minor Injury – Time off unlikely | | | | | | | | **C**  3 = Very likely  2 = Possible  1 = Unlikely or Very Unlikely | | | | | |
| **Hazard Control Measures** | | | | | | | | | | | | | | | | | **Residual Risk** |
| * If there is a risk of damage to property or injury to third parties the working areas are to be segregated; * Ensure that you are familiar with the control measures for the use of podium steps etc. if working at height; * Ensure that routes of access and egress to the work locations are kept clear from tins, tools, materials, waste and debris; * Suitable manual handling techniques are to be used when moving boxes, tins, equipment and materials; * Ensure that the correct PPE is issued and worn including suitable safety gloves, eye protection and any additional PPE which may be included in the site rules. * When sanding and preparation is required ensure that suitable Respiratory Protective Equipment (RPE) is worn correctly by trained operatives in areas of dust exposure; * Ensure that gloves are worn to keep hands isolated from the paint products; * Material Safety Data Sheets and COSHH assessments are to be communicated to operatives to advise them of any specific requirements for the use of PPE/RPE; * Maintain good housekeeping’ Clear up debris and spills as works progress; * Store materials correctly to avoid damage and safely to avoid accidental displacement; * When painting in an existing building, request the asbestos register before commencing work; * Ensure that plugs and switches are isolated and removed by a competent person if they need to be removed prior to painting; * Materials that are not in use are to be stored in a flame proof container if they are flammable and a suitable extinguisher placed next to the box; * Only keep enough materials on site for your work. Do not store large amounts that may add to a fire risk; * Replace lids to tins and thinners etc. that are not in use and store soiled rags in tins to prevent unnecessary fumes and vapour’s; * Never remove paint from the hands using thinners etc. as these types of liquid will pass through skin and cause damage and ill health, dermatitis may also occur; * When using filling knives and craft knives ensure that gloves are worn to protect against injury from cuts; * If sweeping on site use a light sprinkling of water to keep dust down or if possible use a vacuum cleaner. | | | | | | | | | | | | | | | | | **Low**  **(2)** |