|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Assessed By:** | | **Kevin Lovett** | | | | | | | | | **Risk Assessment No:** | | | | | **RA07** | |
| **Hazard Identified:** | | **Ceramic tiling** | | | | | | | | | **Date Reviewed:** | | | | | **June 2025** | |
|  | | | ***A*** | | | | | ***B*** | | | | ***C*** | | | | ***D*** | |
| **Who’s at Risk?** | | | | | **Severity** | | | | **Likelihood** | | | | **Risk Rating** | |
| **E** | | **C** | **P** | | **3** | **2** | **1** | | **3** | **2** | | **1** | **B x C = D** | |
| **🗸** | |  |  | | **🗸** |  |  | |  | **🗸** | |  | **6** | |
| Risk Assessment Ratings | **6-9 High Risk** | | | | | | **4 Medium Risk** | | | | | | | **1-3 Low Risk** | | | |
| **Key** | | | | | | | | | | | | | | | | | |
| **A**  E = Employees  C = Contractors  P = Public / 3rd parties | | | | **B**  3 = Death or Major injury  2 = Reportable injury  1 = Minor Injury – Time off unlikely | | | | | | | | **C**  3 = Very likely  2 = Possible  1 = Unlikely or Very Unlikely | | | | | |
| **Hazard Control Measures** | | | | | | | | | | | | | | | | | **Residual Risk** |
| * Only competent operatives will be employed to complete tiling works; * The work area shall be segregated from third parties; * Where possible ensure the removal of all fixtures and fittings prior to commencement; * Operatives MUST be informed of requirements as prescribed by the COSHH assessments e.g. adhesives, grout, etc.; * Request the asbestos register and location of services prior to works being carried out; * If there is a question with regards to if services are live do not commence work until you have confirmed they are dead; * Ensure the correct PPE is worn to reduce risk as required e.g. suitable safety gloves when there is a risk of cuts, eye protection and hearing protection if using the saw, dust masks when mixing and knee pads when tiling floor areas etc.; * Use suitable manual handling techniques when manoeuvring equipment and materials but in the first instance use the winch or trolleys to move materials. Never lift any loads that may cause you injury; * Do not take too many materials to the work are if it results in reduced access and egress particularly if it is an emergency route; * Ensure that materials and waste never block emergency access and egress routes; * Ensure that tile cutters are checked prior to use and the correct cutting methods are used with any guards in place and correctly set; * Ensure that the work area has good ventilation and there is suitable task lighting to enable you to undertake the task safely; * Check your equipment before use and ensure it has been Portable Appliance Tested (PAT); * Food and drink are not to be consumed in the area where substances such as adhesives or grout are being used; * Ensure adequate ventilation when using adhesives; * Good standards of hygiene are to be maintained. Wash before eating, drinking and going to the toilet. | | | | | | | | | | | | | | | | | **Low**  **(3)** |