|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Assessed By:** | | **Kevin Lovett** | | | | | | | | | **Risk Assessment No:** | | | | | **RA15** | |
| **Hazard Identified:** | | **Slips and Trips** | | | | | | | | | **Date Reviewed:** | | | | | **June 2025** | |
|  | | | ***A*** | | | | | ***B*** | | | | ***C*** | | | | ***D*** | |
| **Who’s at Risk?** | | | | | **Severity** | | | | **Likelihood** | | | | **Risk Rating** | |
| **E** | | **C** | **P** | | **3** | **2** | **1** | | **3** | **2** | | **1** | **B x C = D** | |
| **🗸** | |  |  | |  | **🗸** |  | |  | **🗸** | |  | **4** | |
| Risk Assessment Ratings | **6-9 High Risk** | | | | | | **4 Medium Risk** | | | | | | | **1-3 Low Risk** | | | |
| **Key** | | | | | | | | | | | | | | | | | |
| **A**  E = Employees  C = Contractors  P = Public / 3rd parties | | | | **B**  3 = Death or Major injury  2 = Reportable injury  1 = Minor Injury – Time off unlikely | | | | | | | | **C**  3 = Very likely  2 = Possible  1 = Unlikely or Very Unlikely | | | | | |
| **Hazard Control Measures** | | | | | | | | | | | | | | | | | **Residual Risk** |
| * Operatives must ensure that all trailing leads and cables are hung above head height. If this is not possible then leads and/or cables must be positioned along the skirting line and to avoid door way; * All spillages are to be reported immediately and cleared using the correct equipment to deal with the particular product (refer to the Material Safety Data Sheet and COSHH assessment for substances); * All areas of site must be kept clean and clear of debris; * Operatives shall be appropriately instructed in the importance of reducing slips and trips, maintaining housekeeping and no horseplay; * Operatives are to clear work areas as soon as possible after the waste has been produced. Waste will be recycled. * All waste must be placed into bags and removed to the company vehicle for transportation to a local waste transfer station * Access and egress routes must remain clear at all times and shall not be used as storage areas; * Ensure fire escape routes and exits are kept clear at all times; * There is to be co-operation and co-ordination of activities with all personnel and Site Management to achieve high standards of housekeeping; * Adequate task and general lighting is to be available at all times; * Wear suitable footwear with adequate tread on the sole; * The Supervisor / Foreman shall assess weather conditions which may affect site operations. Particularly during icy, strong winds or heavy rain conditions. | | | | | | | | | | | | | | | | | **Low**  **(2)** |