|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Assessed By:** | | **Kevin Lovett** | | | | | | | | | **Risk Assessment No:** | | | | | **RA06** | |
| **Hazard Identified:** | | **Use of Adhesives** | | | | | | | | | **Date Reviewed:** | | | | | **June 2024** | |
|  | | | ***A*** | | | | | ***B*** | | | | ***C*** | | | | ***D*** | |
| **Who’s at Risk?** | | | | | **Severity** | | | | **Likelihood** | | | | **Risk Rating** | |
| **E** | | **C** | **P** | | **3** | **2** | **1** | | **3** | **2** | | **1** | **B x C = D** | |
| **🗸** | |  |  | |  | **🗸** |  | |  | **🗸** | |  | **4** | |
| Risk Assessment Ratings | **6-9 High Risk** | | | | | | **4 Medium Risk** | | | | | | | **1-3 Low Risk** | | | |
| **Key** | | | | | | | | | | | | | | | | | |
| **A**  E = Employees  C = Contractors  P = Public / 3rd parties | | | | **B**  3 = Death or Major injury  2 = Reportable injury  1 = Minor Injury – Time off unlikely | | | | | | | | **C**  3 = Very likely  2 = Possible  1 = Unlikely or Very Unlikely | | | | | |
| **Hazard Control Measures** | | | | | | | | | | | | | | | | | **Residual Risk** |
| * Ensure an adequate COSHH (Control of Substances Hazardous to Health) assessment has been carried out; * Do not use any substances if you have not been issued with a COSHH assessment; * Ensure all operatives have read and are aware of the risks involved in using these chemicals; * Ensure adequate training and instruction is given on the use of these chemicals; * Ensure any PPE identified in the COSHH assessment is available and worn; * Adhesives and flammable materials are only to be stored on site in steel containers; * Ensure the MSDS (Material Safety Data Sheet) is available, preferably attached to the COSHH assessment and stored in the steel container or an office; * Suitable fire extinguishers are to be placed next to the container at all times; * Ensure adequate ventilation at all times – Use extract ventilation, fans or open doors and windows; * Should anyone complain of dizziness or nausea, immediately remove them to fresh air. If symptoms do not subside within 15 minutes, seek medical attention, and show the medics the MSDS or COSHH assessment and product label if possible; * Ensure that where new, different, substituted or revised products are used, that a new COSHH assessment is carried out and this information is relayed to all operatives. | | | | | | | | | | | | | | | | | **Low**  **(2)** |